;****************************************************************************************
;
; RT2860.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT2860 series Wireless LAN Card.
;
;   Copyright (c)2002-2007, Ralink Technology Corp., All Rights Reserved
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Ralink%
Compatible      = 1
DriverVer       = 01/30/2008, 1.01.01.0000
CatalogFile     = rt2860.cat

[ControlFlags]
;ExcludeFromSelect = PCI\VEN_1814&DEV_0601

[Manufacturer]
%Ralink%        = Ralink, NTamd64
%Sitecom%       = Sitecom, NTamd64
%Edimax%        = Edimax, NTamd64
%Conceptronic%  = Conceptronic, NTamd64
%Planex%        = Planex, NTamd64
%Asus%          = Asus, NTamd64
%D-Link%        = D-Link, NTamd64
%Gigabyte%      = Gigabyte, NTamd64
%AL%            = AL, NTamd64
%Airlink%       = Airlink, NTamd64
%Corega%        = Corega, NTamd64
%Sparklan%      = Sparklan, NTamd64
%ZCOM%          = ZCOM, NTamd64
%Quanta%        = Quanta, NTamd64
%AMIT%          = AMIT, NTamd64
%Foxconn%       = Foxconn, NTamd64
%LITE-ON%       = LITE-ON, NTamd64

[Ralink.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Generic.DeviceDesc%        = RALINK_0601.ndi,      PCI\VEN_1814&DEV_0601
%Generic.DeviceDesc%        = RALINK_0681.ndi,      PCI\VEN_1814&DEV_0681
%Generic.DeviceDesc%        = RALINK_0701.ndi,      PCI\VEN_1814&DEV_0701
%Generic.DeviceDesc%        = RALINK_0781.ndi,      PCI\VEN_1814&DEV_0781
%Generic.DeviceDesc%        = RALINK_0601.ndi,      PCI\VEN_1814&DEV_0601&SUBSYS_28601814
; MSI
%MSI_6891.DeviceDesc%       = RALINK_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_68911462
%MSI_6890.DeviceDesc%       = RALINK_0781.ndi,      PCI\VEN_1814&DEV_0781&SUBSYS_68901462
; Qcom
%Qcom_6247.DeviceDesc%      = Ralink_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_624718E8
%Qcom_6263.DeviceDesc%      = Ralink_0781.ndi,      PCI\VEN_1814&DEV_0781&SUBSYS_626318E8

[Sitecom.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sitecom_0015.DeviceDesc%   = Sitecom_0601.ndi,     PCI\VEN_1814&DEV_0601&SUBSYS_0015182D
%Sitecom_0016.DeviceDesc%   = Sitecom_0601.ndi,     PCI\VEN_1814&DEV_0601&SUBSYS_0016182D

[Edimax.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Edimax_7728.DeviceDesc%   = Edimax_0601.ndi,       PCI\VEN_1814&DEV_0601&SUBSYS_77281432
%Edimax_7708.DeviceDesc%   = Edimax_0601.ndi,       PCI\VEN_1814&DEV_0601&SUBSYS_77081432
%Edimax_7758.DeviceDesc%    = Edimax_0601.ndi,      PCI\VEN_1814&DEV_0601&SUBSYS_77581432
%Edimax_7738.DeviceDesc%    = Edimax_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_77381432
%Edimax_7748.DeviceDesc%    = Edimax_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_77481432
%Edimax_7768.DeviceDesc%    = Edimax_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_77681432
%Edimax_7727.DeviceDesc%    = Edimax_0701.ndi,      PCI\VEN_1814&DEV_0701&SUBSYS_77271432

[Conceptronic.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic_3C85.DeviceDesc% = CONCEPTRONIC_0601.ndi,  PCI\VEN_1814&DEV_0601&SUBSYS_3C851948
%Conceptronic_3C86.DeviceDesc% = CONCEPTRONIC_0601.ndi,  PCI\VEN_1814&DEV_0601&SUBSYS_3C861948
%Conceptronic_3C90.DeviceDesc% = CONCEPTRONIC_0701.ndi,  PCI\VEN_1814&DEV_0701&SUBSYS_3C901948
%Conceptronic_3C91.DeviceDesc% = CONCEPTRONIC_0701.ndi,  PCI\VEN_1814&DEV_0701&SUBSYS_3C911948

[Planex.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Planex_ED07.DeviceDesc%    = Planex_0601.ndi,      PCI\VEN_1814&DEV_0601&SUBSYS_ED0714EA
%Planex_ED09.DeviceDesc%    = Planex_0601.ndi,      PCI\VEN_1814&DEV_0601&SUBSYS_ED0914EA
%Planex_ED08.DeviceDesc%    = Planex_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_ED0814EA

[Asus.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Asus_130F.DeviceDesc%      = Asus.ndi,             PCI\VEN_1814&DEV_0601&SUBSYS_130F1043
%Asus_130E.DeviceDesc%      = Asus.ndi,             PCI\VEN_1814&DEV_0601&SUBSYS_130E1043

[D-Link.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%D-Link_3C0A.DeviceDesc%    = D-Link.ndi,           PCI\VEN_1814&DEV_0601&SUBSYS_3C0A1186
%D-Link_3C43.DeviceDesc%    = D-Link.ndi,           PCI\VEN_1814&DEV_0601&SUBSYS_3C431186

[Gigabyte.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Gigabyte_E937.DeviceDesc%  = Gigabyte_0601.ndi,    PCI\VEN_1814&DEV_0601&SUBSYS_E9371458
%Gigabyte_E938.DeviceDesc%  = Gigabyte_0681.ndi,    PCI\VEN_1814&DEV_0681&SUBSYS_E9381458
%Gigabyte_E939.DeviceDesc%  = Gigabyte_0681.ndi,    PCI\VEN_1814&DEV_0681&SUBSYS_E9391458
%Gigabyte_E93A.DeviceDesc%  = Gigabyte_0681.ndi,    PCI\VEN_1814&DEV_0681&SUBSYS_E93A1458
%Gigabyte_E93B.DeviceDesc%  = Gigabyte_0781.ndi,    PCI\VEN_1814&DEV_0781&SUBSYS_E93B1458

[AL.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AL_3C89.DeviceDesc%        = AL.ndi,               PCI\VEN_1814&DEV_0601&SUBSYS_3C891948
%AL_3C8A.DeviceDesc%        = AL.ndi,               PCI\VEN_1814&DEV_0601&SUBSYS_3C8A1948

[Airlink.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Airlink_3C87.DeviceDesc%   = Airlink_0601.ndi,     PCI\VEN_1814&DEV_0601&SUBSYS_3C871948
%Airlink_3C88.DeviceDesc%   = Airlink_0601.ndi,     PCI\VEN_1814&DEV_0601&SUBSYS_3C881948
%Airlink_3C8C.DeviceDesc%   = Airlink_0701.ndi,     PCI\VEN_1814&DEV_0701&SUBSYS_3C8C1948
%Airlink_3C8D.DeviceDesc%   = Airlink_0701.ndi,     PCI\VEN_1814&DEV_0701&SUBSYS_3C8D1948

[Corega.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Corega_C124.DeviceDesc%    = Corega_0601.ndi,      PCI\VEN_1814&DEV_0601&SUBSYS_C1241259
%Corega_C129.DeviceDesc%    = Corega_0601.ndi,      PCI\VEN_1814&DEV_0601&SUBSYS_C1291259
%Corega_C12A.DeviceDesc%    = Corega_0601A.ndi,     PCI\VEN_1814&DEV_0601&SUBSYS_C12A1259

[Sparklan.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sparklan_0022.DeviceDesc%  = Sparklan_0601.ndi,    PCI\VEN_1814&DEV_0601&SUBSYS_002217F9
%Sparklan_0023.DeviceDesc%  = Sparklan_0601.ndi,    PCI\VEN_1814&DEV_0601&SUBSYS_002317F9

[ZCOM.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZCOM_0061.DeviceDesc%      = ZCOM_0601.ndi,        PCI\VEN_1814&DEV_0601&SUBSYS_006117CF
%ZCOM_0063.DeviceDesc%      = ZCOM_0601.ndi,        PCI\VEN_1814&DEV_0601&SUBSYS_006317CF

[Quanta.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Quanta_0300.DeviceDesc%    = Quanta_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_03001A32
%Quanta_0503.DeviceDesc%    = Quanta_0681.ndi,      PCI\VEN_1814&DEV_0681&SUBSYS_05031A32

[AMIT.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AMIT.DeviceDesc%           = AMIT.ndi,             PCI\VEN_1814&DEV_0601&SUBSYS_050018EB

[Foxconn.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Foxconn_E002.DeviceDesc%   = Foxconn_0781.ndi,     PCI\VEN_1814&DEV_0781&SUBSYS_E002105B

[LITE-ON.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%LITE-ON_6600.DeviceDesc%   = LITE-ON_0781.ndi,     PCI\VEN_1814&DEV_0781&SUBSYS_660011AD
%LITE-ON_7600.DeviceDesc%   = LITE-ON_0781.ndi,     PCI\VEN_1814&DEV_0781&SUBSYS_760011AD

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[RALINK_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[RALINK_0681.ndi]
AddReg                  = PCI0681.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[RALINK_0701.ndi]
AddReg                  = PCI0701.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[RALINK_0781.ndi]
AddReg                  = PCI0781.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Sitecom_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Edimax_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Edimax_0681.ndi]
AddReg                  = PCI0681.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Edimax_0701.ndi]
AddReg                  = PCI0701.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CONCEPTRONIC_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CONCEPTRONIC_0701.ndi]
AddReg                  = PCI0701.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Planex_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Planex_0681.ndi]
AddReg                  = PCI0681.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Asus.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[D-Link.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Gigabyte_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Gigabyte_0681.ndi]
AddReg                  = PCI0681.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Gigabyte_0781.ndi]
AddReg                  = PCI0781.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[AL.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Airlink_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Airlink_0701.ndi]
AddReg                  = PCI0701.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Corega_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Corega_0601A.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg, IEEE80211H.reg, CarrierDetect.reg
CopyFiles               = win9x.CopyFiles

[Sparklan_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[ZCOM_0601.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Quanta_0681.ndi]
AddReg                  = PCI0681.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[AMIT.ndi]
AddReg                  = PCI0601.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Foxconn_0781.ndi]
AddReg                  = PCI0781.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[LITE-ON_0781.ndi]
AddReg                  = PCI0781.ndi.reg, RT28609X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RALINK_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RALINK_0681.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RALINK_0701.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RALINK_0781.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Sitecom_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Edimax_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Edimax_0681.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Edimax_0701.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CONCEPTRONIC_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CONCEPTRONIC_0701.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Planex_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Planex_0681.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Asus.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[D-Link.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Gigabyte_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Gigabyte_0681.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Gigabyte_0781.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AL.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Airlink_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Airlink_0701.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Corega_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Corega_0601A.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg, IEEE80211H.reg, CarrierDetect.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Sparklan_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ZCOM_0601.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Quanta_0681.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIT.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Foxconn_0781.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[LITE-ON_0781.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

; NT services sections
[RALINK_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[RALINK_0681.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[RALINK_0701.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[RALINK_0781.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Sitecom_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Edimax_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Edimax_0681.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Edimax_0701.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[CONCEPTRONIC_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[CONCEPTRONIC_0701.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Planex_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Planex_0681.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Asus.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[D-Link.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Gigabyte_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Gigabyte_0681.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Gigabyte_0781.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[AL.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Airlink_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Airlink_0701.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Corega_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Corega_0601A.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Sparklan_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[ZCOM_0601.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Quanta_0681.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[AMIT.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[Foxconn_0781.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[LITE-ON_0781.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Block ACK settings
;
HKR, ,                            BACapability,      0x10001, "0x07034040"
HKR, Default,                     BACapability,      0x10001, "0x07034040"


;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting,      0x10001, "0x2BA15"
HKR, Default,                     TransmitSetting,      0x10001, "0x2BA15"


;
; Country Region G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region 11G"
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, "#0 (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,    1,                  0, "#1 (Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum,    2,                  0, "#2 (Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum,    3,                  0, "#3 (Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum,    4,                  0, "#4 (Channel 14)"
HKR, NDI\params\CountryRegion\enum,    5,                  0, "#5 (Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum,    6,                  0, "#6 (Channel 3 - 9)"
HKR, NDI\params\CountryRegion\enum,    7,                  0, "#7 (Channel 5 - 13)"

;
; Country Region A Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, "Country Region 11A"
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "0"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, "#0 Ch(36 - 64,149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,1,                 0, "#1 Ch(36 - 140)"
HKR, NDI\params\CountryRegionABand\enum,2,                 0, "#2 Ch(36 - 64)"
HKR, NDI\params\CountryRegionABand\enum,3,                 0, "#3 Ch(52 - 64,149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,4,                 0, "#4 Ch(149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,5,                 0, "#5 Ch(149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,6,                 0, "#6 Ch(36 - 48)"
HKR, NDI\params\CountryRegionABand\enum,7,                 0, "#7 Ch(36 - 165)"
HKR, NDI\params\CountryRegionABand\enum,8,                 0, "#8 Ch(52 - 64)"
HKR, NDI\params\CountryRegionABand\enum,9,                 0, "#9 Ch(36 - 116,132 - 165)"
HKR, NDI\params\CountryRegionABand\enum,10,                0, "#10 Ch(36 - 48,149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,11,                0, "#11 Ch(36 - 120,149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,12,                0, "#12 Ch(36 - 140)"

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "5"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,              0, "1"
HKR, NDI\params\TXBurst,                ParamDesc,      0, "TX Burst"
HKR, NDI\params\TXBurst,                type,           0, "enum"
HKR, NDI\params\TXBurst,                default,        0, "1"
HKR, NDI\params\TXBurst\enum,           0,              0, "Disable"
HKR, NDI\params\TXBurst\enum,           1,              0, "Enable"

;
; Enable TGnWifiTest Mode
;
HKR, ,                            TGnWifiTest,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"
HKR, NDI\params\AdhocOfdm,              ParamDesc, 0, "Adhoc Wireless Mode"
HKR, NDI\params\AdhocOfdm,              type,      0, "enum"
HKR, NDI\params\AdhocOfdm,              default,   0, "1"
HKR, NDI\params\AdhocOfdm\enum,         0,         0, "802.11 B Only"
HKR, NDI\params\AdhocOfdm\enum,         1,         0, "802.11 B/G Mix"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
HKR, NDI\params\BGProtection,           ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection,           type,      0, "enum"
HKR, NDI\params\BGProtection,           default,   0, "0"
HKR, NDI\params\BGProtection\enum,      0,         0, "Auto"
HKR, NDI\params\BGProtection\enum,      1,         0, "On"
HKR, NDI\params\BGProtection\enum,      2,         0, "Off"

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "0"
HKR, NDI\params\FrameAggregation,       ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation,       type,      0, "enum"
HKR, NDI\params\FrameAggregation,       default,   0, "0"
HKR, NDI\params\FrameAggregation\enum,  0,         0, "Disable"
HKR, NDI\params\FrameAggregation\enum,  1,         0, "Enable"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, "IEEE802.11h"
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, "Disable"
HKR, NDI\params\IEEE80211H\enum,  1,               0, "Enable"

;
; CarrierDetect
;
HKR, ,                               CarrierDetect,   0, "0"
HKR, NDI\params\CarrierDetect,       ParamDesc,       0, "Carrier Detect"
HKR, NDI\params\CarrierDetect,       type,            0, "enum"
HKR, NDI\params\CarrierDetect,       default,         0, "0"
HKR, NDI\params\CarrierDetect\enum,  0,               0, "Disable"
HKR, NDI\params\CarrierDetect\enum,  1,               0, "Enable"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, "Auto Channel Select"
HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
HKR, NDI\params\AutoChannelSelect\enum,  0,        0, "Disable"
HKR, NDI\params\AutoChannelSelect\enum,  1,        0, "Enable"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "1"
HKR, NDI\params\WMMCapable\enum,        0,         0, "Disable"
HKR, NDI\params\WMMCapable\enum,        1,         0, "Enable"

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "0"
HKR, NDI\params\APSDCapable\enum,       0,         0, "Disable"
HKR, NDI\params\APSDCapable\enum,       1,         0, "Enable"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "0"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BE\enum,         1,         0, "Enable"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "0"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BK\enum,         1,         0, "Enable"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "0"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VI\enum,         1,         0, "Enable"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "0"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VO\enum,         1,         0, "Enable"

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"
HKR, NDI\params\MaxSPLength,      ParamDesc,       0, "Max Service Period Length"
HKR, NDI\params\MaxSPLength,      type,            0, "int"
HKR, NDI\params\MaxSPLength,      default,         0, "0"
HKR, NDI\params\MaxSPLength,      min,             0, "0"
HKR, NDI\params\MaxSPLength,      max,             0, "3"
HKR, NDI\params\MaxSPLength,      step,            0, "1"
HKR, NDI\params\MaxSPLength,      optional,        0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"
HKR, NDI\params\DLSCapable,             ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable,             type,      0, "enum"
HKR, NDI\params\DLSCapable,             default,   0, "0"
HKR, NDI\params\DLSCapable\enum,        0,         0, "Disable"
HKR, NDI\params\DLSCapable\enum,        1,         0, "Enable"

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "0"
HKR, NDI\params\SmartScan,              ParamDesc, 0, "SmartScan"
HKR, NDI\params\SmartScan,              type,      0, "enum"
HKR, NDI\params\SmartScan,              default,   0, "0"
HKR, NDI\params\SmartScan\enum,         0,         0, "Disable"
HKR, NDI\params\SmartScan\enum,         1,         0, "Enable"

;
; RDG
;
HKR, ,                            RDG,             0, "1"
HKR, NDI\params\RDG,                    ParamDesc, 0, "RDG"
HKR, NDI\params\RDG,                    type,      0, "enum"
HKR, NDI\params\RDG,                    default,   0, "1"
HKR, NDI\params\RDG\enum,               0,         0, "Disable"
HKR, NDI\params\RDG\enum,               1,         0, "Enable"

;
; AllowBW40InBGBand
;
HKR, ,                            AllowBW40InBGBand,      0, "1"
HKR, NDI\params\AllowBW40InBGBand,      ParamDesc, 0, "AllowBW40InBGBand"
HKR, NDI\params\AllowBW40InBGBand,      type,      0, "enum"
HKR, NDI\params\AllowBW40InBGBand,      default,   0, "1"
HKR, NDI\params\AllowBW40InBGBand\enum, 0,         0, "Disable"
HKR, NDI\params\AllowBW40InBGBand\enum, 1,         0, "Enable"

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, "Disable"
HKR, NDI\params\PSPXlink\enum,    1,               0, "Enable"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Initialize Delay
;
HKR, ,                            InitDelay,     0x00010001, 0x00080000

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
;HKR, ,                            SSID,            0, %SSID_DEF_STR%
;HKR, Default,                     SSID,            0, %SSID_DEF_STR%
;HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
;HKR, NDI\params\SSID,             type,            0, "edit"
;HKR, NDI\params\SSID,             limitText,       0, "32"
;HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""
HKR, NDI\params\Networkaddress,   optional,        0,  "1"

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "1"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "1"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

[IEEE80211H.reg]
HKR, ,                IEEE80211H,      0, "1"

[CarrierDetect.reg]
HKR, ,                CarrierDetect,   0, "1"

[PCI0601.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0601"

[PCI0681.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0681"

[PCI0701.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0701"

[PCI0781.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0781"

[RT28609X.ndi.reg]
HKR, ,                            NTMPDriver,       0, RT28609x.sys

HKR, ,                            BusType,          0, 5
HKR, NDI,                         CardType,         0, "PCI"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "RT28609x.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "RT28609X"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
XP.CopyFiles            = 12    ; system32\drivers subdirectory on Windows XP
win9x.CopyFiles         = 11    ; system subdirectory on win9x

[NT.CopyFiles]
rt2860.sys                        ; NT Installation

[XP.CopyFiles]
rt2860.sys

[win9x.CopyFiles]
rt28609x.sys                      ; Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt2860.sys                = 1
rt28609x.sys              = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RT80x86.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "RT80x86"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2860.sys
LoadOrderGroup              = NDIS


[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2860.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[Strings]
Ralink                      = "Ralink Technology, Corp."
Sitecom                     = "Sitecom Europe BV"
Edimax                      = "Edimax Technology Co., Ltd"
Conceptronic                = "Conceptronic"
Planex                      = "Planex Communications, Inc."
Asus                        = "ASUSTeK Computer Inc."
D-Link                      = "D-Link"
Gigabyte                    = "Gigabyte Technology Corp."
AL                          = "AL Tech., Inc."
Airlink                     = "Airlink"
Corega                      = "corega"
Sparklan                    = "Sparklan Communications, Inc."
ZCOM                        = " "
Quanta                      = "Quanta Microsystems, Inc."
AMIT                        = "AMIT Technology, Inc."
Foxconn                     = "Foxconn"
LITE-ON                     = "LITE-ON TECHNOLOGY CORPORATION"

;*******************************************************************************************
; Device description
;*******************************************************************************************
Generic.DeviceDesc          = "802.11n Wireless LAN Card"
Sitecom_0015.DeviceDesc     = "Sitecom Wireless-N Network PC Card WL-180"
Sitecom_0016.DeviceDesc     = "Sitecom Wireless-N Network PCI Card WL-181"
Edimax_7728.DeviceDesc      = "Edimax 802.11n PCI Card"
Edimax_7708.DeviceDesc      = "Edimax 802.11n Cardbus Card"
Edimax_7758.DeviceDesc      = "Edimax 802.11n Wireless mini PCI Card"
Edimax_7738.DeviceDesc      = "Edimax 802.11n Wireless PCIe Cardbus"
Edimax_7748.DeviceDesc      = "Edimax 802.11n Wireless PCIe PCI Card"
Edimax_7768.DeviceDesc      = "Edimax 802.11n Wireless mini PCI Card"
Edimax_7727.DeviceDesc      = "Edimax 802.11n Wireless PCI Card"
Conceptronic_3C85.DeviceDesc = "Conceptronic 802.11n PC-Card (V1)"
Conceptronic_3C86.DeviceDesc = "Conceptronic 802.11n PCI-Card (V1)"
Conceptronic_3C90.DeviceDesc = "Conceptronic 802.11n PC-Card (V2)"
Conceptronic_3C91.DeviceDesc = "Conceptronic 802.11n PCI-Card (V2)"
Planex_ED07.DeviceDesc      = "PCI 802.11n Wireless LAN card bus"
Planex_ED09.DeviceDesc      = "PCI 802.11n Wireless LAN PCI Bus Adapter"
Planex_ED08.DeviceDesc      = "PCI 802.11n Wireless Express Card LAN Adapter"
Asus_130F.DeviceDesc        = "ASUS 802.11n Wireless LAN Card"
Asus_130E.DeviceDesc        = "802.11n Wireless LAN Card"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-645 RangeBooster N650 Notebook Adapter"
D-Link_3C43.DeviceDesc      = "D-Link DWA-547 RangeBooster N650 Desktop Adapter"
Gigabyte_E937.DeviceDesc    = "Gigabyte GN-WI30N 802.11n mini PCI WLAN Card"
Gigabyte_E938.DeviceDesc    = "Gigabyte GN-WP30N 802.11n PCI-E WLAN Card"
Gigabyte_E939.DeviceDesc    = "Gigabyte GN-WS30N 802.11n mini WLAN Card"
Gigabyte_E93A.DeviceDesc    = "Gigabyte GN-WS30HN 802.11n dual-band mini WLAN Card"
Gigabyte_E93B.DeviceDesc    = "Gigabyte GN-WS31N 802.11n mini WLAN Card"
AL_3C89.DeviceDesc          = "AnyGate 11N W-LAN Adapter (XM-240C)" 
AL_3C8A.DeviceDesc          = "AnyGate 11N W-LAN Adapter (XM-241P)"
Airlink_3C87.DeviceDesc     = "Airlink101 300N Wireless CardBus adapter"
Airlink_3C88.DeviceDesc     = "Airlink101 300N Wireless PCI Adapter"
Airlink_3C8C.DeviceDesc     = "Airlink101 Wireless Cardbus Adapter"
Airlink_3C8D.DeviceDesc     = "Airlink101 Wireless PCI Adapter"
Corega_C124.DeviceDesc      = "CG-WLCB144GNL"
Corega_C129.DeviceDesc      = "CG-WLCB144GNL"
Corega_C12A.DeviceDesc      = "CG-WLCB300AGN"
Sparklan_0022.DeviceDesc    = "Wireless Lan 11n CardBus Adapter"
Sparklan_0023.DeviceDesc    = "Wireless Lan 11n PCI Adapter"
ZCOM_0061.DeviceDesc        = "802.11b/g/n Wireless Network Adapter"
ZCOM_0063.DeviceDesc        = "802.11b/g/n PCI Wireless Network Adapter"
MSI_6891.DeviceDesc         = "802.11bgn 2T3R Mini Card Wireless Adapter"
MSI_6890.DeviceDesc         = "802.11bgn 1T2R Mini Card Wireless Adapter"
Quanta_0300.DeviceDesc      = "QMI EM300 11n Wireless LAN Card"
Quanta_0503.DeviceDesc      = "QMI EM503 11n Wireless LAN Card"
AMIT.DeviceDesc             = "802.11n Wireless Mini-PCI Adapter"
Foxconn_E002.DeviceDesc     = "802.11n Wireless LAN Card"
LITE-ON_6600.DeviceDesc     = "Ralink 802.11n Wireless LAN Card"
LITE-ON_7600.DeviceDesc     = "802.11n Wireless PCI Express Card LAN Adapter"
Qcom_6247.DeviceDesc        = "Ralink 802.11n Wireless LAN Card"
Qcom_6263.DeviceDesc        = "Ralink 802.11n Wireless LAN Card"

INSTALL_DISK_STR            = "Ralink 802.11n Wireless LAN Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n Wireless Driver"

; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
;SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11n Wireless Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"

